


Version 2023-01-06



|  |  |  |
| --- | --- | --- |
| **Raspberry Pi GPIO Pin** | **Device** | **Device Pin** |
| 1 | Bosch BME680 Environment Sensor | VCC |
| 3 | SDA |
| 5 | SCL |
| 6 | GND |
| 11 | WaveShare 7.5” ePaper Display | RST |
| 17 | VCC |
| 18 | BUSY |
| 19 | DIN |
| 22 | DC |
| 23 | CLK |
| 24 | CS |
| 39 | GND |
| 29 | Push Buttons | Button 2 |
| 30 | GND |
| 31 | Button 1 |
| 36 | Button 3 |
| 37 | Button 4 |

**Links**<https://www.waveshare.com/wiki/7.5inch_e-Paper_HAT_Manual#Working_With_Raspberry_Pi>   
<https://www.laub-home.de/wiki/Raspberry_Pi_BME680_Gas_Sensor>