
WaveShare eInk Display 7.5"  
170 x 111mm

Optional: PiJuice Battery Pack (12000mAh)  
130 x 70 x 10mm

BME680  
16 x 32mm


Ø 2mm

USB Power Plug



WaveShare Display Controller  
65 x 30mm

Ø 2.5mm



Raspberry Pi Zero 2  
(Optional: PiJuice Battery Controller)  
65 x 30mm

Push Buttons  
69 x 20mm

Ø 8mm drill hole, countersunk to 10mm (inside-out)

Ø 4mm

Version 2023-01-03

Pi Weather Display Base Plate  
210 x 150mm

Plexiglas Base Plate