

Ø 4mm

Ø 8mm, countersunk to 10mm (inside to outside)



WaveShare Display Controller  
65 x 30mm

Ø 2.5mm



Raspberry Pi Zero 2  
(Optional: PiJuice Battery Controller)  
65 x 30mm

Version 2022-11-14

Pi Weather Display Base Plate  
210 x 150mm

Optional: PiJuice Battery Pack (12000mAh)  
130 x 70 x 10mm

WaveShare eInk Display 7.5"  
170 x 111mm

Plexiglas Base Plate